|  |  |  |  |
| --- | --- | --- | --- |
| ITEM | PRICE  | SIZING  | COMMENTS |
| Patches, “Maine Bureau of Parks and Lands” Full Color Logo |  | N/A | * Approved proof required. No work to proceed without Departmental approval.
* 2 patches per jacket (1 per sleeve). Patches to be provided by vendor. Patch dimensions: 3.5” wide by 3.75” tall. See attached image.
* All patches to be seam sealed during jacket production.
 |
| Back Placards w/Reflective Applique |  |  | * Velcro attachment on rear of jackets.
* Background Color: Forest (Material Code 9131)
* Placard 1: “MAINE STATE PARKS” (see attached “Back Placards” for specifications)
* Placard 2: “ALLAGASH RANGER” (see attached “Back Placards” for specifications)
 |
| Cascadia Rain Jacket |  | XXS – 5XL | * Color: Forest (Material Code 9131)
* 2-way waterproof pit zips
* Main front waterproof zip
* Front left chest pocket
* Patches sewn on, seam sealed in production
* As per attached specifications.
 |
| Cascadia Rain Pant |  | XXS – 5XLShort, Regular, Tall | * Color: Black (Material Code 9131)
* Full leg side zips
* As per attached specifications.
 |
| Dolomite Jacket |  | XXS – 5XL | * Color: Forest (Material Code 9131)/Black (Material Code 2321)
* 3L Waterproof stretch fabric
* Patches sewn on, seam sealed in production
* Back zipper vent w/Velcro under flap
* Reflective piping on arms, front and back, width ¼”
* Cover over main front zipper placket
* As per attached specifications.
 |
| Green Mountain Softshell |  | XXS – 5XL | * Color: Forest/Black
* Reflective piping on front and back yoke, width ¼”
* Back placket for placard w/Velcro
* Patches sewn on, seam sealed in production
* Zip-off sleeves
* As per attached specifications.
 |
| Isobar Parka w/Zip-out 100g Thinsulate Insulation |  | XXS – 5XL | * Color: Forest (Color 9131)/Black (Color 2384)
* 20,000 dpm waterproofing / 20,000 breathability
* Reflective piping on front and back yoke, width ¼”
* Back vent for placard w/Velcro
* Patches sewn on, seam sealed in production
* As per attached specifications.
 |
| 100g Thinsulate Jacket Insulation |  | XXS – 5XL | * Color: Black
 |
| 200g Thinsulate Jacket Insulation |  | XXS – 5XL | * Color: Black
 |