|  |  |  |  |
| --- | --- | --- | --- |
| ITEM | PRICE | SIZING | COMMENTS |
| Patches, “Maine Bureau of Parks and Lands” Full Color Logo |  | N/A | * Approved proof required. No work to proceed without Departmental approval. * 2 patches per jacket (1 per sleeve). Patches to be provided by vendor. Patch dimensions: 3.5” wide by 3.75” tall. See attached image. * All patches to be seam sealed during jacket production. |
| Back Placards w/Reflective Applique |  |  | * Velcro attachment on rear of jackets. * Background Color: Forest (Material Code 9131) * Placard 1: “MAINE STATE PARKS” (see attached “Back Placards” for specifications) * Placard 2: “ALLAGASH RANGER” (see attached “Back Placards” for specifications) |
| Cascadia Rain Jacket |  | XXS – 5XL | * Color: Forest (Material Code 9131) * 2-way waterproof pit zips * Main front waterproof zip * Front left chest pocket * Patches sewn on, seam sealed in production * As per attached specifications. |
| Cascadia Rain Pant |  | XXS – 5XL  Short, Regular, Tall | * Color: Black (Material Code 9131) * Full leg side zips * As per attached specifications. |
| Dolomite Jacket |  | XXS – 5XL | * Color: Forest (Material Code 9131)/Black (Material Code 2321) * 3L Waterproof stretch fabric * Patches sewn on, seam sealed in production * Back zipper vent w/Velcro under flap * Reflective piping on arms, front and back, width ¼” * Cover over main front zipper placket * As per attached specifications. |
| Green Mountain Softshell |  | XXS – 5XL | * Color: Forest/Black * Reflective piping on front and back yoke, width ¼” * Back placket for placard w/Velcro * Patches sewn on, seam sealed in production * Zip-off sleeves * As per attached specifications. |
| Isobar Parka w/Zip-out 100g Thinsulate Insulation |  | XXS – 5XL | * Color: Forest (Color 9131)/Black (Color 2384) * 20,000 dpm waterproofing / 20,000 breathability * Reflective piping on front and back yoke, width ¼” * Back vent for placard w/Velcro * Patches sewn on, seam sealed in production * As per attached specifications. |
| 100g Thinsulate Jacket Insulation |  | XXS – 5XL | * Color: Black |
| 200g Thinsulate Jacket Insulation |  | XXS – 5XL | * Color: Black |